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Danger Zones & Blind Spots

Scope
This guide indicates optimum separation distances between our most common
moving plant and people and also identifies common blind spots.

Other plant has danger zones and blind spots which we should be aware
of prior to starting work (e.g. pavers, millers, cranes, etc).

DIAGRAM KEY

Bxra distance ovtside rear danger zone:

Danger zone area Continued danger zone area Extend danger zone to
displayed in metres when the truck deck is up height of deck when tipping

n Bitumen tankers

Front 10m, sides 8m, rear 15m (deck up, over 15m)

Dump trucks and ADT's
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